* Remove 3 unused holes under the DC to DC converter
* Add support holed for the DC to DC converter